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1.0 
(i) 

- Site organization is an exercise done to produce a layout of the site that is logical, ordinary and above all practical. Site layout plan shows the proposed locations of all facilities, accommodation and plant area to secure optimum economy, efficiency and safety during construction.

(ii)

· To ease movement of plant on site for the cost effectiveness, efficient and economic operation of the equipment.
(iii) 

· Cement should be stored in a building or shed that is dry, leak proof and as moist proof as possible.

·  The building should be free from draughts which can bring in moist air and may cause an air set (hardening) of the cement. The building should be well ventilated.
· Cement should not be stored directly on the ground as it would become damp

· Cement should be stacked off the floor on wooden planks so as to provide a clearance from the floor of 150 to 200mm and a minimum space of 450mm around between the exterior walls and the stacks.
· Cement bags should be placed close together to minimize the circulation of air within the stack.

· Cement should not be stored for long periods on site. The manager should facilitate rotational use so that the material being used comes from the older stock.

· In humid climate, cement should not be stored for more than two months before use.

· Cement storage during monsoon or in humid areas the stack shall be enclosed completely with proofing membrane.

· The width of a stack is to be restricted to 4 bags length or 3 meters, and to prevent the possibility of lumping under pressure, restrict the height of the stack to 15 bags.
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(iv)

- By coating the steel with cement wash before stacking.
- By storing the steel above ground level by at least 150mm upon platforms.

(v)
- Exit control helps in site protection against vandalism.
- Maximum security requirements necessitate the inspection of vehicles entering or leaving the premises.

- Access control for labor staff and visitors to site.

2.0
- For site protection against theft of tools, materials and small equipment.
- Acts as a deterrent to would be trespassers or thief.

- Defines the limits of the site.

3.0

- Mainly outdoor electrical installations are open to the sky or partially covered.

- Unprotected from environmental hazards as compared to installations in buildings.
- Require special consideration as they are characterized by frequent modifications. 
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