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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	Please insert your completed assignment ( in word format)  here:
1. Give short answers for the following questions: (20)
i. What do you understand by the term ‘site organization’? 
ii. Highlight the importance of preparing the site road suitable for the movement of heavy construction equipment.
iii. List the precautions to be taken for the storage of cement at a construction site. 
iv. What will you do to prevent scaling and rusting of structural and reinforcing steel?
v. How does exit control help in site protection?
2. Discuss the advantages of providing fences for construction sites (5) 
3. How is the provision of site electricity different from building electricity? (5)

1.
i.           Construction organization is method to boosting effectiveness and efficiency of construction works using layout plan. All site amenities are placed in a way so construction could run as smoothly as possible to increase productivity and quality of works strictly following health and safety rules. 
ii.          It is very important to prepare suitable road for site operation since construction uses a lot of different types of heavy machinery starting from HGV lorries to mobile cranes weight of which can reach 150 tons. Appropriately prepared road also helps to easy site congestion, preparing loading and unloading bays decreases increase loading and offloading time.
iii.         Although concrete buildings are very durable, cement in its raw form it is very delicate material and a lot of factors can reduce its qualities or even make it useless. Cement must not be kept in basement, and should be stored in dry area, at least 150 to 200 millimeters above ground with impermeable protective sheeting underneath and 600 millimeters away from any wall and other individual cement pile. 
iv.         To eliminate chances of structural and reinforcement steel corrosion this steps must be taken; good quality steel must be used and reputable manufacturer that can prove its quality, corrosion resistant coating must be used, good quality cement that contains anticorrosive agents with reputable manufacturer who cam its quality, and use of high quality experienced work force.
[bookmark: _GoBack]v.            Site exit plays very important role in construction. Provision of site exit control eliminates chances of equipment and materials being stolen from site, accountability for number of people making sure no one left behind in an emergency.  
2.            
               Construction site is very hazardous environment therefore fence used to serve few purposes: 
Fence barriers are used around its perimeter to eliminate chances of public wandering into site, construction workers use designated entrance for access control.
Fence barriers are used for security purposes to eliminate risk of theft of tools, materials and equipment. 
Contractor can use advertisement on fences to promote it amongst public. 
3.
              Construction site uses temporary method such as diesel generators to provide itself with electricity for project life cycle or temporary connection to power grid through formal agreement from local authorities. Also majority of construction equipment use 110V to operate to reduce chances of electric accidents. 
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