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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.

For high grades use examples and illustrations where appropriate. 
	1. Give short answers for the following questions: 

I. What is the use of fusible webbing?
Fusible web is a man made fiber that will melt when heated. When placed between two pieces of fabric, the melting action of the web causes it to fuse the fabrics together. It is not woven or knitted. Fusible web is available in rolls, similar to tape, in various widths, by the yard in the interfacing department of most fabric stores and in pre-packaged pieces.

Fusible web is used for hemming or for bonding two layers of fabric together; it is available in narrow strips for hems, or in 18″ (46 cm) widths for fusing larger areas.
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II. How should the fabric storage area be organized?
Fabric storage area should be organized or categorized in different ways both for keeping them safe or keeping them orderly.
To maintain an ordered room the area could be categorized:

· By Colour: whites, blues, tans, reds, greens, etc.
· By Style: plaid, stripe, toile, polka dots, floral, contemporary graphics, holiday, etc.

· By Texture: cotton, rayon, denim, velvet, silk, canvas, leather, etc.

· By Purpose: fashion clothing, crafts, etc.

III. Why it is important to have a separate fabric storage area for storing patterns?
It is important to have a seperate storage area for storing patterns as it will help to be tidy and ordered to find a specific pattern.

They could be stored as the way a designer find easy like as storing them in plastic container, baskets etc. The way we store them will help us to find and use them as necessary. It is also important to label them by the desired way such as storing them by style, size, gender, could be useful.

III. What is the difference between diagonal basic stitch and dress maker basting stitch?
Diagonal basting: Diagonal basting is a series of parallel, horizontal stitches that produce diagonal floats of thread on the top layer of fabric. This stitch is most often used in tailoring to hold fabric layers together (not along a stitching line). The stitches control the shifting of fabric during pressing, fitting and construction. Diagonal basting is perfect for holding a pocket in place, so it doesn’t shift during stitching. But in dressmaker basting the way is taking one long and two or three short stitches is the method. 
[image: image2.jpg]



[image: image3.jpg]



2. Define the followings: 

Hemming, combination stitch, back stitching, shirring, gathering, gauging, whipping
Hemming

In hemming, turn in the edge of the fabric ¼ inch, then turn second time, and baste to

under fabric. Make small slanting stitches from right to left, catching only a thread or two

of the under material. A bias hemming tape may be stitched on to avoid turning hem

under. Blind hemming is done like hemming but with larger stitches through the fold and

only one thread on under side. The work is invisible on the right side. This too can be done

more rapidly with a sewing machine and is especially recommended when considerable

hemming is to be done. Slip stitching is done for very fine work and is invisible on both sides. Take up one thread on underside of fold and one on underside of fabric.
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A combination stitch is two running stitches followed by one backstitch. It is stronger than a straight running stitch, but not as strong as backstitching.
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Backstitching Backstitch is most easily worked on an even-weave fabric, where the threads can be counted to ensure regularity, and is generally executed from right to left. The stitches are worked in a 'two steps forward, one step back' fashion, along the line to be filled, as shown in the diagram.

Neatly worked in a straight line this stitch resembles machine stitching.

The back stitch can also be used as a hand-sewing sewing utility stitch to attach two pieces of fabric together.
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Gathering is a sewing technique for shortening the length of a strip of fabric so that the longer piece can be attached to a shorter piece. It is commonly used in clothing to manage fullness as when a full sleeve is attached to the armscye or cuff of ashirt, or when a skirt is attached to a bodice.

In simple gathering, parallel rows of running stitches are sewn along one edge of the fabric to be gathered. The stitching threads are then pulled or "drawn up" so that the fabric forms small folds along the threads. 
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Shirring is two or more rows of gathers that are used to decorate parts of garments, usually the sleeves, bodice or yoke. The term is also sometimes used to refer to the pleats seen in stage curtains.
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Gauging uses 2-3 rows of synchronized running stitch (even or uneven), but the stitches are worked close to the folded waist edge of a freshly-balanced skirt. The drawn-up gauged pleats are laid right-sides-together with a finished waistband or bodice, and each rounded “valley” that touches the band or bodice is hand-whipped to the finished edge. This creates a “hinge” that pushes the skirt out and away from the body when worn. Because no fullness is enclosed in the waistband, or resting on the inside of the bodice, gauged skirts add zero to very, very minimal bulk at the waist.
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3. Explain the following types of seams and where each of the following seam is used? 

Whipped seam, curved seam, strap seam, lapped hem stitched seam, tucked seam
Whipped seam The whipped seam can be made by two method. Both are variation of the plain seam. The first method used on transparent fabric like chiffon, silk mousseline, and organza, is strong and looks more like a heavy cord then a seam.

1. Right sides together, baste and stitch a plain seam; remove the bastings and press the seam flat. Baste the seam allowance 2 mm. away.

2. Fold both seam allowance over on the basting. Baste again on the stitched line.

3. Overcast the folded edge.
 
4. Trim the seam allowance close to the overcasting, using the "palm up" technique-hold the seam in one hand in slip the blade of your 13 mm. trimmers under the row edge. 
Keeping both palms up and the scissors almost parallel to the garment minimises the possibility of snipping into the stitching.

The alternate method in a softer seam then the one above, but since it isn't suitable for fabric that fray badly or for closely fitted designs, it should only be used for seams that will not to be stressed.

1. Baste and stitch a 15 mm. seam, right sides together.Stitch again 3 mm. away.Press the seam flat.

2. Trim close to the second row of stitching and overcast the trimmed seam.
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Curved seam must be clipped or slashed in several places to make it lie flat. This is important for smooth finish.

Strap seam The strap seam is a hallmark of couture construction. Its only function is decorative, but it can add interest to an otherwise plain garment. 
From there, cover the plain, and the lined curved strap seam, shown in the photo. This seam is beautiful for use in constructing princess seams, because of the extra emphasis it adds to the lines of the garment.
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Lapped seam This type of seam is frequently used on nonwoven fabrics, suchas synthetic suede and leather, as well as real suede and leather, because their edges do not fray.

Trim away the seam allowance on one of your squares. This will be the “upper” section of the seam.

Lap the upper section over the second fabric square, placing the trimmed edge along the lower square’s seamline; hold it in place with hand basting, double-faced basting tape, glue stick or fuse basting.

Edgestitch along the trimmed edge, going through both upper and lower layers. Topstitch on the overlap 1/4" (6mm) away from the first stitching line, again going through both layers of fabric.
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Hemstitched seam is a decorative drawn thread work or openwork hand-sewing technique for embellishing the hem of clothingor household linens. Unlike an ordinary hem, hemstitching can employ embroidery thread in a contrasting color so as to be noticeable.

In hemstitching, one or more threads are drawn out of the fabric parallel and next to the turned hem, and stitches bundle the remaining threads in a variety of decorative patterns while securing the hem in place. Multiple rows of drawn thread work may be used.[1]

 HYPERLINK "https://en.wikipedia.org/wiki/Hemstitch" \l "cite_note-RD78-2" [2]
[image: image14.jpg]



Tucked seam is similar to lapped seam except that the final stitching is done not at the edge, but at a distance from the fold. The effect is like that of a tuck.
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