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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	



 1. Give short answers for the following questions:                                                                                
 
I. What is the use of fusible webbing?  
 It is a sticky bonding that adheres two fabrics together and it comes in many different bands, each being slightly different. Most fusible webbing have paper on one side, some have paper on both sides, while others have no paper at all.


II. How should the fabric storage area be organized?
 It should be organized according to the material and the color on shelves that it show the fabrics

III. Why it is important to have a separate fabric storage area for storing patterns?
          To not being confusing between fabrics and pattern.


        IV. What is the difference between diagonal basic stitch and dress maker basting stitch?  
        The diagonal basic stich is used for materials that fray easily, be they thick or thin. It is also a good stitch to use for seams that get hard wear or extra strain (waistlines and armholes) and also for narrow seams. Make the plain seam fist then press seam open and work casting stitches over any raw edges of the two seam allowances separately
And the dress maker basting stich is Temporary stiches are sometimes referred to as tacking stiches, They are usually horizontal and sewn from left to right with a knot. It is a better idea to use a contrast colour thread for tacking. 




2. Define the followings:


Hemming:
 is used to secure down a folded edge of material hems. This will appear as small, slanting stitches on the right and wrong side. This stitching should be spaced close enough to hold the hem securely and should be firm but also far enough apart so it’s not noticeable from the right side of the garment. Fasten the thread with a few tiny stitches on top of each other before starting the hem. To finish off the hemming, use several stitches to make sure it is fastened securely. 


Combination stitch:
With this combination, a backstitch and three or four running stitches are used, in particular for working plain seams that are done by hand. This is a stich which is stronger than the running stitch and faster than the backstitch.


Back stitching:
This type of stitching is sometimes substituted for machine stitching and is very strong. The stitching is about 1/16 to 1/8 inch long on the topside. This stitch is made by pushing the needle up through the material on the stitching line about 1/8 inch from the right end. Insert the needle 1/8 inch back of the thread at the beginning of the stitching line then bring it out an equal distance in front of the thread. Keep going like this and make sure the stitches are uniform in size and quite firm.

Shirring:
is gathering of an area of fabric by means of drawn or elasticized threads in parallel rows which are used for a decorative finish. This can be a decorative feature on the waistline, shoulder, or the lower part of a sleeve. Shirring is usually at the parts of a garment that are narrower so this also gives room for a certain amount of stretching. The rows must be equally spaced. Shirring can be done in two ways: thread shirrs and elasticized shirrs.


Gathering: To achieve a decorative and very effective method of distributing fullness over a particular area, use a gathering. They provide fullness and create a soft look. They are also very graceful. A machine can be used to make the gathers or they can be done by hand. Draw the fabric together on a line of stitching. Gathers are used to control fullness around the waist, neckline, yoke line, and upper and lower edges of sleeves.


Gauging:
It’s the same meaning of shitting.

Whipping:
is mostly used for joining a gathered or unaltered section to a straight edge, usually as in a yoke. Take the part that is to be laid on top and turn its seam allowance to the wrong side. Place this piece on top of the second piece making sure the right sides are facing. Match the fold to the seam line. Tack in position and machine close to the folded edge.




3. Explain the following types of seams and where each of the following seam is used?       

   Whipped seam
It also called A lapped seam is mostly used for joining a gathered or unaltered section to a straight edge, usually as in a yoke. Take the part that is to be laid on top and turn its seam allowance to the wrong side. Place this piece on top of the second piece making sure the right sides are facing. Match the fold to the seam line. Tack in position and machine close to the folded edge.

curved seam
Edge Stitched Finish This is when the seam is stitched and pressed open (Fig.10.4b). Turn under ¼ inch on each seam edge and top stitch near the fold without catching the garment. This finish is not appropriate for deeply curved seams as it is quite a bulky finish which is mostly used on unlined jackets or coats.

Strap seam
This seam is usually used down the centre front and centre back of coats, dresses, and skirts and is a variation of the lapped seam. This seam will give the piece of clothing a decorative effect when the fabric of the backing piece stitched in between is a different colour. You can machine baste on the seamline and this will leave long threads on each end. Press open the seam and cut 1 ½ inch wide underlay of fabric which is the same or a contrasting fabric. Centre it under seam and baste.





Lapped hem stitched seam
A counter seam is durable and used for men’s wear and reversible pieces which use very thick material. There are two methods of doing this: 
Method I Turn down a small portion of the wrong side of a fabric and also on the right side of the other piece. Iron them strongly. Take the first piece on the wrong side and the second piece on the right side making sure to maintain the seam allowances then tack them in position. Use a machine to stitch it along the folded edges. This is a three-layered counter seam.
 Method II Using the wrong side of a piece, turn it down 0.5cm and take the right side of the other piece. Iron them firmly. Keep the wrong side of the first piece on the right side of the second piece. Move the turned down edges under each other then pin them in position and tack them. Using the machine, stitch along the folded edges from the right and wrong sides, This is a four-layered counter seam.


Tucked seam
[bookmark: _GoBack]For the stitching of tucks it is necessary to fold along the middle so that the stitching lines correspond and stitch along the markings. Only when the stitching of the tucks is finished should the garment section be cut. There are a few ways of tucking and these include:














Student Statement:

By submitting this assignment, I confirm that this is my own work.



	Student Signature
	
	Date
	




For Tutor / Assessor Use Only
	Total Marks
	

	Marks Obtained
	

	Percentage / Grade
	













image1.png
ﬁ
o R




