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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	
Assessment 12

Question 1


a.) The flat pattern method is necessary for the areas like pants or sleeves.

I. 
b.) The draping pattern method helps the designer to; See proportion and lines of the design exactly as they will look three dimensionally on the wearer.

     c.)  Pattern grading decides; How patterns increase or decrease in sizes

 

Question 2


a.) Dart – help shape the flat piece of fabric into a form-fitting one that fits the curves of the human body. Also damage or broken stitching lines meet at a point to create the dart, it shows as well line where to fold the fabric to create dart.

          Grain line -  is a symbol of straight line that may or may not have arrows head              
           at each end. It is more important for pattern marking.


        Hemline -  Direction on the pattern shows the recommended finished length of     
        the project, which varies from person to person.


Question 3

a.) Selvages – are the parallel to the lengthwise grain, a finished edges where the fabric comes off the looms.

Lengthwise Grain – On knit fabrics, the lengthwise grain in usually more stable and less stretchy than the crosswise grain while grain line run length of the fabric, parallel to the selvages.
           
           Bias – 45 degress between the lengthwise and crosswise grains. When you    
           pull a woven fabric on the bias it stretches and is very malleable. Bias as well   
           can be easily to shaped to follow a curved edge.



Question 4

a.) Placing the pattern pieces on grain: The grain line allows you to cut the piece on-grain, meaning that the pattern piece lines up with the lengthwise grain of the fabric.
     
         First Step: Fid and cut apart the paper pattern pieces you need to make your     
                          project view; set aside them. Trace the pattern size you need on        
                          pattern tracing paper, remember to transfer all the pattern markings 
                          from the master pattern. Cut the paper pattern pieces apart, don’t 
                          cut them out right on the cutting line, leave a little of the paper past 
                          the cutting line, to get easy and faster when you get it on the fabric.
 
          
                          Locate the lengthwise grain or place on folds symbols on the paper      
                          pattern piece. Use the flat table, before laying the pattern in the   
                          tissue on the fabric, mark symbols using a highlighter for easy        
                          reference.

                           Lay the fabric on the table, If the fabric is longer than your table or                 
                           cutting board, prevent the excess fabric weight from stretching and   
                           pulling on your fabric by folding it and laying it on the end of the  
                           table.

                           Making sure that the grain line is parallel to the selvages. Check             
                           each pattern piece in placed precisely on grain by poing a pain 
                           straight down into the grain line, measuring the distance straight 
                           across from on end on to the line to the selvage. Be sure to pivot  
                           the paper pattern so that each of the pattern pieces is equidistant         
                           from the selvage.



b.) Pinning and Cutting out the pieces – It is a pin the pattern pieces, doubled layer of fabric so that the pins go through both fabric layers are perpendicular. This prevents the fabric from shifting during the cutting process.

          First Step:  No need to pin every inch, just pin at the notches everywhere the   
                            pattern changes direction.

                             O long, straight edges, such as pant legs and sleeves seams, 
                             place pin every 4 inches. Cut out your pattern pieces using a pair   
                             of sharp dressmaker’s shears.

                             For accurate cut in the middle of the solid cutting line marked on  
                             the pattern tissue, trying not to lift the fabric off the table too much  
                             when cutting. For the beginner constructing a project you transfer 
                             the pattern marks indicating darts, tucks, pleats, and the other  
                             symbols to your fabric pattern pieces for a very good reason.

                             Example: when marking a pleat, tuck, or dart, instead of marking  
                            the entire stitching line, simply mark the dots on the stitching lines. 
                            When you put the right sides together for swing, pin the project 
                            together for sewing, pin the project together by matching the dots; 
                            sew from dot to dot (pin to pin).
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