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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	
Assessment 13

Question 1


I.) Fusible web is used for hemming or for bonding two layers of fabric together; it is available in narrow strips for hems, or in 18” (46 cm) widths for fusing larger areas.

I. 
II.) First to organized the fabric are make a thorough inventory list of all the items you need in your sewing room such as;

Sewing machine           Dress Forms
Sewing table                 Garment steamer
Fabric                            Cutting board
Patterns 
Treads
mirror
Notions: thimbles, threads, tracing tools, needles, pins, cushions, bobbins, elastic, seam rappers, pins, ribbon, dyes, fabric care.

III.)  It is very important to have a separate fabric storage area for storing patterns, to   
             maintain the fabric beauty especially for the vast collection

                  Also to make it sure that you can care the fabrics better to categorized them by:
  
                  Color : separate in different color such as, white, blue, tans, reds, green, etc

               Style: plaid, strip, toile, polka dots, floral, contemporary graphics, holiday etc
               Texture: cotton, rayon, denim, velvet, silk, canvas, leather, etc
               Purpose: fashion clothing, crafts, etc

               It is very important as well to safely store the fabric

               Neatly folding and place in plastic containers. Put label on it by cutting small  
               swatches on each fabric.
 
               Use multi-tiered hangers with clips to help prevent the wrinkles and lest space.

               In a large Ziploc bag it is advisable as well to put small fabric.

IV.) The differences of Diagonal basic stitch and dress maker basting stitch;

Diagonal basting is using to prevent slipping of material when inserting zippers or putting in coat linings.

Slant stitches on right side from bottom to top, come through to wrong side, hold needle in a straight line and pull out to right side again directly below where you originally inserted needle.

While Dressmaker basting take one long and two or three short stitches.


Question 2


a.) Hemming – turn in the edge of the fabric ¼ inch, then turn second time, and baste to under fabric.

bias hemming tape may be stitched on to avoid turning them under while blind hemming is done like hemming with large stitched through the fold and only one thread on under side.

           Back stitching – it is a strongest handmade stitch.

           Shirring – is the effect gotten by two or more rows of gathering. Make two or three        
           lines of running stitches not more that ¼ inch apart and holding all the ends together, 
           gather fasten threads around a pin.

           Gathering – it is an effect not a stitch.

           Gauging - bring a large amount of material into a small space. Two or three lines of  
           uneven basting, making sure that corresponding stitches lie directly in line, one above 
           the other, pull up threads as in gathering and shirring.

           Whipping - done to get a fine finished edge. Roll edge to be whipped a little at a 
           time, wrong side facing you, hold roll tightly, and make tiny slanted stitches that pass 
           under not through the roll.     
        
      


Question 3

      Whipped Seam –  used for piecing when fabric is not wide enough to cut full pattern. 
       Make it sure that the grain of piecing is the same as the grain of garment/sawing project, 
        turn in edges and overcast with tiny stitches.

      Curved Seam – must be clipped or slashed in several places to make it lie flat. When it  
       comes to smooth finished this is very important

      Strap Seam – used for decoration.

      Lapped hem stitched Seam – done by lapping seams, hemstitch over the 
       basting, trim away seam on wrong side.

[bookmark: _GoBack]      Tucked Seam – similar to lapped seam except that the final stitching is done not at the  
        edge, but at a distance from the fold. Effect is like that of a tuck
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