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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	Please insert your completed assignment (in word format) here: 

i. The term Site organisation can be described as a detailed and well thought out plan which ensures efficient, effective, healthy and safe construction site throughout its build. Furthermore, it requires producing a site layout which is practical, logical, and orderly. In the process of site organisation, the following factors must be considered: site accommodation, security, machinery, material, site drainage, storage, site electricity, lighting, labour, and access to site and site roads.

ii. The importance of preparing the site road suitable for movement of heavy construction equipment is significant in order to achieve and maintain a rapid tempo of construction in all weathers. For example, the construction project will be delayed if the heavy equipment is stuck in one place due to the poor road condition, therefore causing unnecessary cost and time overruns.




iii. The following precautions must be to be taken to store cement at a construction site:
· Store cement in a building which must be dry, moist-proof and leak-proof. 
· Adequate ventilation must be provided in the storage building in order to prevent dampness.
· Stack Cement on wooden planks with a gap of about 150-200mm from the floor. 
· Leave a minimum spacing of about 450mm between the walls and the stacks.
· Pack the cement bags together to reduce circulation of air within a stack and a width limit of 4 bags and height of 15 bags per stack to prevent lumping under pressure.
· The rule of first-in, first-out should be followed. Older stocks should be utilized first to avoid prolonged storage.
· Do not store cement for more than two months in humid climatic conditions. 
· To store cement for long periods in humid areas, the stack must be covered with waterproof materials. 

iv. Structural and reinforcing steel should be coated with cement wash before stacking to prevent rusting and scaling. They should also be stored in such a way to avoid distortions and to prevent deterioration and corrosion. In addition, they should be sorted based on the different types and sizes and stored separately on platforms which are more than 150mm above ground as per BIS guidelines.

v. Exit control is important for construction site protection because it facilitates the safety and security of the personnel, equipment and materials on site. Only authorised persons, vehicles and equipment are allowed to access or exit the site. It also enables spot checks on personnel in order to verify the number of persons still at the job site. In addition, exit control also helps to take the appropriate actions in the event of a security violation at the site. For example, the suspected violator is apprehended and detained at the exit point until help arrives.

2. 
Construction site fence is a temporary installation that mark the limits of clearing, grading and defining areas to be protected. The fence serves two major functions which are outlining the limit of the site as well as providing protection against losses and theft. Fencing a construction site provides many advantages such as providing a physical restriction or serving as a visual barrier for ongoing construction works. 
The fence also helps in providing security for administrative offices, since these buildings usually contain valuable gadgets and documents for administrative and site management purpose. The necessary security measures should therefore be put in place to prevent criminals from getting easy access to the site administrative building. For example, we can hear of thefts and trespassing incidents occurring during the night at construction sites whereby construction equipment and building materials are stolen and sold on the black market.

In addition, there are cases where hooligans or terrorist sneak into construction sites with the aim of simply damaging everything within their reach. These acts of sabotage will often end up costing the construction company a lot of money in damages on restoration. 
Furthermore, providing fences for construction sites can prevent criminals and trespassers from entering the site or clearly seeing a property. This can result in a reduced ability to invade privacy, or plan and commit a person or property crime. In addition to these benefits, site fencing also offers the site owners controlled access to their site and clear boundary demarcation.





3. 
The provision of electricity on a construction site is to provide lighting and power to enable the works to be carried out. By the temporary nature of the situation, the installation will be subjected to the kind of ill treatment which is unlikely to be applied to most fixed building installations. For example, workers on the site may be ankle deep in mud and thus particularly susceptible to a shock to earth, and they may be using portable tools such as drills and grinders in situations where danger is more likely than in most factory building situations. 
Furthermore, the main issues confronting construction sites with regards to electrical installation is the unprotected nature of the outdoor installations which makes them potential hazards. Short circuiting and exposure to live wires could result in fires or shocks respectively. Building electricity supply is permanent in nature and it is well protected and regulated.
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