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	Assignment 05
1. 
i. Site organization basically involves setting up a site layout which comprises of the practical, logical, and orderly arrangement of plants, facilities, and equipment. 
ii. Site road preparation should be carried out to create: 
· Ready access to firefighting, equipment and first aid services in cases of an accident.
· Roads must be maintained to prevent potholes and ditches from developing and damaging vehicles
· In situations where on-off site vehicles attempt to use on-site roads, adequate signs and supervision must be provided for safety reasons.
iii. The precautions required to be taken for the storage of cement at a construction are as follows:
· Cement must be stored in a building which must be dry-proof, moist-proof, and leak-proof.
· Adequate ventilation must be provided to prevent dampness
· The cement bags should be neatly packed to reduce circulation of air within a stack.
· Old stocks should be utilized first to avoid prolong storage.
· Cement procured to be stored for long periods in monsoon or humid areas, should be covered with waterproof materials
iv. To prevent scaling and rusting of structural and reinforcing steel, the steel should be coated with cement wash before stacking.
v. How does exit control help in site protection? separate exit and entry points would aid on-off movement of traffic at the site

2. Providing fences for construction sites serves the following purposes on a construction site.

· It serve as a means of protecting the site against losses and theft.
· It outlines the limit of the site
· It serve as a means of providing physical restriction from trespassers
· It can also serve as visual barriers during open work construction

3. The differences between site electricity and building electricity are as enumerated below:

· Site electricity is required for a short time during the period of construction and it might not be connected to the main power source while the building electricity supply is well connected to an electrical supply pole and has a link to the national grid for proper metering. 
· Site electricity is required to provide power for gadgets and lighting for accommodation and to power different types of machinery.
· [bookmark: _GoBack]The main sources of power to a construction site are grid supply from the local authority and portable generators while the building will require connection from grid to the homes via permanent electric poles.
· It is more convenient to go for the permanent supply from the local authority since the structure being constructed would eventually require this source of power supply using permanent supply cables
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