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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	Please insert your completed assignment ( in word format)  here:

                                                      SEWING BASICS
                                                     ASSESSMENT 13

1, Fusible webbing; is used for hemming or for bonding two layers of fabric together, it is available in narrow strips for hems, or in 18[44cm] widths for fusing larger area. Or is a fiber that will melt when heated when placed between two pieces of fabric the melting action of the fusible web causes it to fuse the two fabrics together.  
 
i, Fabric storage area should be organized; It will help these fabrics maintain their beauty and structure by storing them safely, By folding neatly and place in plastic containers, label the outside by cutting small swatches of each fabric.
By hanging fabric in a closet with a skirt or pant hanger, multi-tiered hanger with clips can save space and help prevent wrinkles.
By placing smaller amounts of fabric in large Ziploc bags.   

iii, Is important to have separate fabric storage area for storing patterns; by storing them separate  it helps in keeping both the fabric and the pattern neat and tidy at all time. 
By storing them separate also help in organizing them 
Storing the fabric and pattern separate helps in reaching any fabric or pattern you need to use at the time you need to use it.
Storing fabric and pattern separate also help in creating more space, like pattern should be fold neatly in a drawer or keep pattern tucked inside a sturdy photo box, plastic containers, pretty rectangular baskets, label the drawer or boxes based on the style, size, gender male or female.
Fabric could be stored by hanging them on hanger, by placing smaller amount of fabric in large Ziploc bags, by folding them neatly and place them in plastic containers label the outside by cutting small swatches of each fabric.  

iv, The difference between diagonal basic stitch and dress maker basting stitch is; 
Diagonal basic stitch is used to prevent slipping of material when inserting zippers or putting in coat linings, is also a series of parallel horizontal stitches that produce diagonal floats of thread on top layer of fabric, is mostly used in tailoring to hold fabric layers together.

Dress maker basting; take one long and two or three short stitches also temporally sew with long removable stitches which is removable once permanent sewing is done.

2, Hemming is fabric that is turned up on the lower edge of a garment or sleeve to provide a finished edge 

Combination stitch, is the style that combines by inserting the needle through the back leg rather than through the front leg without twisting the stitch.
 
Back stitching, is a stitch made by inserting the needle at the midpoint of a preceding stitch so that the stitches overlap by half lengths on the back of the fabric and appear continuous on the front, Or a stitch in which the thread is doubled back on the preceding stitch. 

Shirring; Is a magical technique for sewing texture that takes a regular piece of fabric and shrinks it up giving it elasticity or sewing with elastic thread in the bobbin of sewing machine to create a smocked appearance on the fabric.

Gathering; is a technique used to bunch together a length of fabric to create a ruffled effect or when stitching thread are then pulled or drawn up so that the fabric forms small fold along the threads.

Gauging; is used to bring a large amount of material into a small space do to two or three lines of uneven basting making sure that corresponding stitches lie directly in line one above the other, pull up thread as in gathering and shirring. Is also typically reserved for handling skirt fullness and develops as a common technique in the early to middle 1840s when increasing skirt circumferences and fashion preference. 

Whipping; is done to get a fine finished edge, is to sew together two separate pieces of material with flat edge.

4, Whipped seam is another variation of plain seam, the whipped seams looks more like a heavy cord then a seam.
And is used for piecing when fabric is not wide enough to cut full patter. Sewing project, turn in edge and overcast with tiny stitches

Curved seam;  is for clipped or slashed in several places to make it lie flat’
Is used for smooth finish. 

Strap seam; is used for decoration, plain seam is made and pressed on the right side baste a strip of material with edges turn in, and stitches both sides braid and other trimmings may also be used.   

Lapped hem; ; is two or more piles of material are lapped that is with edge overlaid plain or folded and joined with one or more rows of stitches. Is used by turning one piece o material under on the seam allowance, baste the folded edge on to the right side of the piece at seam allowance will look like a fall seam when finished
 
Stitched seam is the join where two or more layers of fabric or material are held together with stitch. Is used with variety of techniques to prevent raveling of raw fabric edges and to neaten the inside of garments.  

Tucked seam; is a seam in which the edge of the upper ply, folded along the seam line forms a tuck, a tucked seam is a decorative seam there two layers of fabric join there is a tuck of smooth transition. 
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