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Question 1

I, What do you understand by the term site organization ?
Site to be practical, logical and orderly.

II, High light the importance of preparing the site road suitable for the movement of heavy construction equipment?
To ensure more effective, economic operations also to reduce mud and debris being transferred on to the highways which will then become a safety issue to the public.

III, List the precautions to be taken for the storage of cement at a construction site?
Stored in a dry building moist proof and leak proof to be put on planks with a gap of about 150 to 200mm from the floor and 450mm from walls and other stacks. To be stacked on top of each other to reduce circulation no more than 4 wide and 15 bags high.

IV, What will you do to prevent scaling and rusting from reinforcing steel?
Coat the steel in cement wash before stacking and then stack 150mm from off the ground.

V, How does exit control help site protection?
Helps to inspect vehicles leaving the site.

Question 2,
 Discuss the advantages of providing fences for construction sites?
Prevents as best possible vandalism, theft and losses, a more defined boundary from the public and better controls health and safety on the site.

Question 3,
How is the provision of site electricity different from building electricity?
[bookmark: _GoBack]The main issue are confronting electrical installation are the unprotected nature of the outdoor installation that make a potential hazard. But the site can have a Tempary Builder Supply (TBS) installed from the main electricity supplier to ensure a safer supply to the sites needs 


    



