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	1.
I). Site organization means is layout that is logical, orderly and practical and is it shows 
     proposed positions of facilities such as accommodation, ablutions, site offices and
     site location.

ii).  The importance of preparing the site road suitable for the movement of heavy 
       construction equipment, this will help for easy access for delivery vehicles, for
       efficient movement of haulage trucks to spoil sites, suitable site roads also helps to
       protect the environment because vehicles will use designated routes whereas if
       there are no roads drivers tend to use any available short routes without considering
       environment in an area. The use of un designated routes may lead to damage or
       destruction of some protected species.

III). Precautions to be taken for the storage of cement at a construction site are:
       Must be stored in a shade, dry and area that does not allow moisture penetration
       In a ventilated area and must not be stored direct on the ground as it would become
       Damp. Cement should not be stored for more than two months before use.

IV). Structural and reinforcing steel must be coated with cement wash before staking to 
       prevent scaling and rusting.

V).  Exit control help in site control, it limits the movement of vehicles on site as they
      are controlled when they exit. Exit control on site also help to manage risks of accidents
      and damages to the environment and surrounding structures.


2).The advantages of providing fencing for construction sites are:
   a). It protects vandalism of plant and theft of materials within the site.
   b). It restricts random access into site
  c).  Fencing protects animals and people from falling into deep excavation during works.
  d).  Fencing demarcates the site and will help to see the extend of the site
  e). Acts as a deterrent to the would be trespasser or thief.
  f). The other advantage is that fencing helps to control in and out vehicles since there
       will all use one entrance and exit.

3). Electricity supply for site is always an outdoor electrical installations open to sky or 
      Partially covered whereas for buildings electricity is an indoor and always covered.
[bookmark: _GoBack]      Site electricity is generally unprotected from environment hazards whereas for
      For buildings is protected fully from environment.
  For buildings there are special considerations during installation whereas site electricity
  Its done to suit requirements for that time only without due considerations of future.
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