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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	1. Answer the following questions: 
i. What are the economic objectives of quality control how are they achieved?
Every construction project seeks to build a structure at the least cost and of a high quality. A high quality structure can be achieved at lower cost if the following costs are minimized or reduced:
i. Failure cost due to quality issues with materials or products which may result in rework, scrapping, low productivity on the field or even spoilage of items
ii. Appraisal cost inherent in conducting quality control assurance using testing, inspection and
other means of product evaluation
iii. Prevention costs associated with avoiding mistakes during construction. 
These costs are linked to personnel training, quality control engineering and maintenance of equipment. Some economic reasons for undertaking quality control include:
i. Cost savings by minimizing rejects or rework
ii. Cost savings by keeping within boundary of design specifications and not extending beyond
iii. Savings obtained by making quality product at no extra cost to parties involved in the project Savings will happen when the contractor engages the services of well-trained supervisors, when he maintains a high standard of specifications and also when the contractor understands that good quality control will improve on the profitability of the project.
ii. What are the features of field quality control?
Field quality control requires the use of equipment, employees’ expertise and other facilities depending on the quality measure stipulated in the contract. It is the responsibility of the lab manager to evaluate equipment requirements and deployment during quality control checks. The number of personnel required to perform quality control inspection and testing will depend on the workload and scheduling of activities on the field. It is best to wait and perform quality control measurements after the peak periods of activities when more workers become available. To ensure quality control measures are effectively, it is important to perform priority ratings for each activity to differentiate between the most and least vital activities. Priority is given to activities having the highest rating first when carrying out quality control procedures.
Field quality control usually involves:
i. The desire to provide an excellent service
ii. Discovering the most effective way of performing tasks
iii. Making use of experience to get things done
iv. Being proud of effort one makes to get tasks accomplished
v. Providing business opportunity for the contractor
vi. The owner getting joy and satisfaction from having value for money
iii. How can contractor quality control be implemented effectively?
The contractor’s quality control plan is vital to assure the project owner(s) that everyone involved is aware of the steps needed to achieve a high quality product. The quality control plan of the contractor is usually discussed by all participants before work begins. It is neither meant to control activities of the contractor nor to pry into his affaires but to endure everybody understand why it is important to maintain good quality control measure at all times.
iv. Why are specifications important?
Specification deals with the quality of work being undertaken in the field using the right quality of materials. Limits are set on the physical properties of materials for quality control purposes. If a quality control inspector finds that a representative sample of a particular material being tested or evaluated falls outside the specified limits, the material from which the sample was taken may be rejected if successive tests show all results are outliers or fall outside the limits. It is the prerogative of the designer to specify what is an acceptable or an unacceptable result from the beginning. Statistical and probability tools may be used for evaluation of samples and determining the quality of materials being used on the field. When a sample falls outside specifications, the whole batch or lot from which it was taken may be rejected.
v. What are incentives and penalties in specifications?
Restrictions are normally imposed on the contractors to prevent them from rushing to complete the project ahead of schedule. This safeguard the project in terms of quality control objectives as specified in the contract. Penalties in the form of fines are sanctioned against the contractor if he fails to follow the specified procedures. Incentives are provided for compliance with laid down procedures. Both penalties and incentives are included in contracts, but it is advisable to avoid including penalties because they tend to strain the relationship between the owner and the contractor.
2. How can you achieve quality control in the field? 
Quality control in the field must be carefully planned to achieve the best quality product at minimal cost using techniques as diverse as those required to carry out specific activities on the field. Developing a good quality control plan requires asking the following questions and finding the right answers to them:
i. Which aspects of quality work are required to be executed?
ii. When is the ideal time to execute each activity during construction?
iii. What methodology or procedure should be used to accomplish these activities?
iv. Who should be responsible for the work in the field?
v. Where specifically, should the work be executed?
vi. What tools, equipment or instruments are required?
vii. What inputs are required to get the structure completed, i.e. what materials and information
is required?
viii. What is the expected end result of the quality control testing? Will the result of the test prompt
decisions to be made and what criteria are available for this decision-making process?
ix. Would the results of the tests warrant the identification and routing of materials?
x. Should records of action be kept and in what format?
xi. What alternatives procedure should be used when differences exist in the product quality?
xii. Will there be a time limit for carrying out quality control and what will that be?


3. What are the advantages and disadvantages of contractor quality control'?
Advantages :
i. When testing and inspection are integral part of the project, then the cost can be wellmanaged by the contractor
ii. The contractor is in a stronger position to anticipate problems and take the necessary steps to adjust the work to solve the problem
iii. The contractor is better placed to build quality into the product than the owner’s quality control supervisor
iv. Testing by the contractor can help him improve on his performance or efficiency at a relatively lower cost
v. Integrating statistical specification into the contractor’s daily activity and displaying this information for other workers to view on daily basis will yield better overall quality
vi. Disputes between the contractor, suppliers and quality control department may be avoided if all quality issues are made the sole responsibility of the main contractor
vii. There will be more time available to the owner’s quality control team to focus on solving more general problems on the site.
Disadvantages:
i. The contractor may not have enough capacity to perform satisfactory quality control programs
ii. Contractor quality control is only suitable when the end pint specifications are available. However, not all projects have end pint specifications due to incomplete project plans
iii. Well-trained quality control experts will be required to assist the contractor to meet quality control targets. But unfortunately, there are very few personnel with these kind of skills Factors affecting implementation of contractor quality control:
i. Quality control is only successful when the contractor has the mind to integrate it into the product
ii. If the personnel working in the field are of a high calibre, the work becomes high quality, especially when the personnel are very experience and highly educated
iii. The owner should clearly specify that he requires the services of a high calibre of quality control personnel so that the contractor will make the effort to recruit supervisors with the right kind of skill
iv. There should be separation of quality control and production function and having quality control team report directly to the site manager instead of the contractor to ensure integrity of standards
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