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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	Please insert your completed assignment ( in word format)  here:
1a. ii
1b.i
1c ii


2a
A dart is a fold in a piece of fabric. Darts give shape to fabric and ensure that patterned flat fabric follows the shape of the body.

Reference:
https://en.wikipedia.org/wiki/Dart_(sewing)


The grain line is the orientation of the thread of the fabric. The most common grainline directions are horizontal and vertical.

Reference:
https://en.wikipedia.org/wiki/Grain_(textile)



The hem line is the lower edge of a piece of clothing, e.g., the bottom of a skirt, or a pair of trousers. 
Reference:
https://en.wikipedia.org/wiki/Hemline

3a.
Selvages are the finished edges where the fabric comes off the looms.
They are parallel to the lengthwise grain.

References:
http://levistrauss.com/unzipped-blog/2014/04/17/those-oft-forgotten-pant-parts/
Page 4, Working with patterns handout, Brentwood College

The lengthwise grain means the direction of the threads in fabric when it is parallel to the selvage.

Reference:
https://www.youtube.com/watch?v=gAtdRPXbn3U

The bias is a line or cut of a fabric that is at 45 degrees across the grain of the fabric.

Reference:
https://sewdifferent.co.uk/cutting-fabric-on-the-bias/


4a.

’Placing the pattern pieces on grain’

1. Cut the paper for your project. Trace the pattern onto tracing paper if you need to make the item in a different size. Ensure that all the pattern markings are transferred. Cut a bit further from the actual lines when cutting out the actual pieces, to make it quicker and easier to put them onto the fabric.
2. Find the lengthwise grain or place-on-fold symbols and mark the symbols before putting the tissue on the fabric on a flat surface.
3. Fold the fabric and put it on the 
flat surface (preferably a table or cutting board). If the fabric is too long, fold it and place it at the end of the board/table so that it doesn't pull or stretch.
Lay out the pattern on-grain and make sure the grain line is parallel to the selvages.
A pin can be used to make sure that each piece is placed exactly on the grain. The pin should be placed into the grain line and the distance across one end of the grainline to the selvage measured. The distance from the other end of the grainline to the selvage should then be measured.


Reference:
Page 28-29, Working with patterns handout, Brentwood College

 
‘Pinning and cutting out the pieces’

The pattern piece should be pinned to a double-layered piece of fabric, making sure the pins go through both layers. The fabric should be pinned inside the cutting layers. Only the notches and places where the pattern changes direction should be pinned. For long and straight edges, the pins should be placed every four inches. The pattern pieces should be cut with sharp dressmaker's shears in the solid cutting line on the pattern pieces. The fabric should not be lifted from the table too much. Dots, rather than lines should be marked on the stitching line to indicate darts, tucks and pleats etc. When the pieces are reading for sewing, the marked dots should be matched and used to indicate where to pin the garment together. The garment should then be sewn dot to dot (pin to pin).

Reference:
Page 29, Working with patterns handout, Brentwood College
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