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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.

For high grades use examples and illustrations where appropriate. 
	1. Multiple Choice Questions. 

a) The flat pattern method is necessary for the areas like;

ii. Pants or sleeves

b) The draping pattern method helps the designer to;

i. See proportions and lines of the design exactly as they will look three dimensionally on the

wearer

c) Pattern grading decides;

ii. How patterns increase or decrease in sizes

2. Define the followings: 

a) Dart, grain line, hem line

DART: Darts are an essential part of garment construction because they allow flat fabric to take on a shape that will fit the body well. A dart is a folded wedge of fabric that is tapered and stitched down to give shape to a garment. 
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GRAIN LINE:  A guideline in the form of a line or arrow that shows the correct alignment of the pattern of the grain in the material.
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              HEMLINE:  The direction on the pattern shows the recommended finished length of the project, which varies from person to person.
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3. Define the followings: 

a) Selvages, length wise grain, bias

· SELVAGES: A selvage is a self-finished edge of fabric. The selvages keep the fabric from unraveling or fraying. The selvages are a result of how the fabric is created. In woven fabric, selvages are the edges that run parallel to the warp and are created by the weft thread looping back at the end of each row.
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· LENGTH WISE GRAIN refers to the threads in fabric which run the length of the fabric, parallel to the selvedge of the fabric.
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· BIAS is the thread line that is at a forty five degree angle to the lengthwise and crosswise grain of the fabric as it is on the bolt”.
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4. Explain step by step the following processes: 

a) ’placing the pattern pieces on grain’,

Each piece of pattern will show a grain linet hat is also called as lengthwise grain which will allows us to cut the fabric accurately. By following belowmentioned steps a successful placing would be done on grain. 
1. First we have to find proper pattern piece which is necessary fort he Project and cut it apart.  When cutting out the pattern pieces, it would be better to leave an extra paper which will help us to cut out paper pieces faster and easier when we use the fabric.
2. Secondly, we have to pay attention to the location of lengthwise grain to the paper pattern pieces. Marking over these symbols using a highlighter will help much before laying the pattern tissue on the fabric.

3. Now we are ready to fold and then lay the fabric on a table by using the instructions on the pattern guide. We have to prevent the excess weight fabric from pulling or strecthing our fabric which will cause wrong cut if our fabric is longer than the area we used. 
4. Again using the pattern guide for following the suggested layout, we need to lay out the pattern on grain. We have to pay attention that the grain line must be parallell to the selvages.

5. Now it is time to pin one end of the grainline arrow to hold it in place and we need to measure from the pinned end of the arrow to the fabric selvage edge and also measure from the other end of the grainline arrow to the fabric selvage edge. Make sure it is the same distance from the selvage as the end we have already pinned in place.  By adjusting the distance and then pinning the arrow in place we will be ready to  pin the edges of the pattern piece in place.
6. Pin with care to prevent inaccurate cutting. A cutting error of ⅛ inch on each side of a pattern piece can result in a ½ inch difference in the final garment. 

7. Use only enough pins to hold down the pattern securely. Depending on the fabric and the size of the pattern piece, placing pins about four inches apart is usually enough. 

8. Place pins completely inside the cutting line. Place pins diagonally in corners. 

9. Use pattern weights instead of pins to hold the pattern in position, if desired. However, be sure to pin grainlines in place first. Position weights, inside the cutting lines, on one pattern piece at a time.
10. Use sharp shears or a rotary cutter to cut out your pattern pieces. Never use pinking shears. Pattern pieces cannot be cut out accurately with pinking shears. 

11. Do not allow the fabric to hang over the edge of the table when you are cutting. This is especially true when working with knits and other stretchy fabrics. The weight of the fabric hanging over the table edge will pull the fabric and result in inaccurate cutting. Also, be careful to leave the fabric resting on the table as you cut. Lifting the fabric will result in inaccurate cutting. 

12. Cut notches out away from the seam allowance. Cutting notches into the seam allowance will weaken the seam. This will also prevent you from letting the seam out if a looser fit is needed. 

13. When using a rotary cutter, always be sure to place a protective plastic cutting mat beneath the fabric. Shift the cutting mat under your work as you proceed around the pattern. A metal ruler can be used as a guide for cutting straight edges. When cutting complex shapes, a small rotary wheel is easier to maneuver than larger ones. You will not be able to cut out the notches with a rotary cutter. Instead, cut off the notches and mark them using another technique, such as chalk or washable marking pen. 

14. Before cutting pattern pieces from a multisize pattern, determine which lines you need to follow. To do this, compare your measurements with those on the envelope size chart. Identify which size you should use for different areas of your body. Use a colored pen to trace along the lines you plan to follow before placing the pattern on the fabric. Taper from the cutting line for one size into the cutting line for another size, as needed. You might also wish to cut out the pattern on the desired size lines before placing it on the fabric.
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