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Marking Criteria:
We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate.
	Please insert your completed assignment ( in word format)  here:


1. Multiple Choice Questions.                                                                                                (3)
a) The flat pattern method is necessary for the areas like;
i. Flowing designs

b) The draping pattern method helps the designer to;
i. See proportions and lines of the design exactly as they will look three dimensionally on the wearer

c) Pattern grading decides;
ii. How patterns increase or decrease in sizes


2. Define the followings:                                                                                                         (9)
a) Dart: In simple terms, darts give shape to otherwise flat fabric. They are the folds that are sewn into the fabric that help the garment better fit the wearer. Every dart has a 'dart point' (the pointed end of the dart) and 'dart intake' (the excess fabric between the lines of the dart).

b) Grainline: The term 'grainline' or 'grain' normally refers to the 'lengthwise grain' which can be found running parallel to the selvedge. The 'grainline' can also be known as the 'warp' on woven fabrics, and the thread that crosses over the warp is called the weft.

c) Hemline: Garments such as coats, skirts and dresses all possess a hemline, which is the the bottom line (or edge) of the garment. Hemlines can come in various shapes and heights depending on the style of the garment; for example, there are above-knee hemlines, floor-length hemlines and mid-calf hemlines.
 

3. Define the followings: (9)
a) Selvedge: A selvedge is the term for the finished edge of traditionally woven-on-the-loom fabric. However, nowadays, selvedges are also found on flat-knitted fabric. The tightly woven edge prevents the fabric from unravelling and runs parallel to the lengthwise grain.

b) Lengthwise grain: The 'lengthwise grain' as stated previously is the grain line that runs parallel to the selvedge. Unlike crosswise grains that can be stretchy, knit fabrics are more stable with lengthwise grains.

c) Bias: The 'bias' grain is the 45 degrees diagonal line between in the lengthwise and crosswise grains on a piece of woven fabric. Bias cut fabric functionally flows better compared to grain that is straight cut because it can stretch and be shaped more easily on edges that are curved.


4. Explain step by step the following processes:                                                                   (9)
a) ’Placing the pattern pieces on grain’: When you want to cut a piece of fabric 'on grain' you will need to use the patterns grain lines that can be found in all pattern pieces. The process of placing the pattern pieces on grain entails:
1.Locate the paper pieces that are needed for your project view and cut them. Once they have been cut place them to one side. If you need to make your desired garment another size do so by using pattern tracing paper and trace your desired size onto the paper as well as all pattern markings from the master pattern. Furthermore, it may help you to be quicker if you cut the pattern lines slightly further along than the real lines.
2.Next, using a flat table, find the 'lengthwise grain' or 'place-on-fold' symbols on the pattern paper and go over them with a highlighter to make them easier for you to find later. Make sure you do this before placing the pattern on the fabric otherwise you could mark your fabric accidentally.
3.Lastly, make sure to follow any pattern guide instructions and lay the pattern (on-grain) onto the fabric making sure the selvedges are parallel to the grain-line. If your fabric is very long it may need slightly folding before placing onto the table or cutting board to prevent it from stretching or pulling.


b) ‘Pinning and cutting out the pieces’: (Before cutting any fabric you will need to obtain a good pair of dressmaker's shears and pins.) Steps on how to pin and cut out fabric:
1.Firstly, to make sure the fabric doesn't move around, pin the selected pattern piece to the fabric by placing the pins perpendicular to/inside the cutting line. If the fabric is double layered, make sure to pin both layers for accurate cutting of both pieces. You do not need to pin all of the fabric as this would be time consuming, instead, only pin the areas where the pattern may change direction or at any notches.
2.Find the solid cutting line on the pattern piece and cut in the middle of it, however, make sure not to lift the fabric too high from the cutting area otherwise this could cause inaccurate cutting.
3.Finally, before taking the pattern off of the fabric make sure you have placed any pattern marks onto the fabric for easier construction of your garment. Moreover, it is not necessary to mark an entire stitching line, instead mark the dots on the lines for stitching and then sew dot to dot.  
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