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Sewing Basics
Unit 13 

1. Give short answers for the following questions;


· What is the use of fusible webbing?
Fusible webbing is a manmade fabric that is used between two pieces of fabrics to glue to each other. So it will stick.

· How should the fabric storage area be organized?
Fabric can be sorted on season, fashion type, craft etc. in plastic boxes. Shoe boxes, plastic bags with a zip on. To prevent any damage to it.

· Why it is important to have a separate fabric storage area for storing patterns? 

Fabric patterns storage can be stored in plastic boxes, shoe box, plastic bags. Just so the pieces of the fabric pattern stay together when needed. 

· What is the difference between diagonal basic stitch and dress maker basting stitch?

Diagonal basic stitch is to prevent slipping of material while inserting a zip.  The dress maker basting stitch takes one, two or three long short stitches. 


2. Define the following;

· Hemming: fold the end of the fabric then fold again press the fabric so it won’t get loose. Stitch the end with needle and thread. Make sure u don’t see much of the thread on the garment.

· Combination stitch:
Two running stitches ended with one backstitch.

· Back stitching: the strongest hand stitch. Stitch up and down continue in a straight line up and under. 

· Shirring: to get the effect of shirring you will have to stitch two rows or more at least ¼ inch apart with running stitches and pull from the end to create shirring.
· 
· Gathering: Gathering is used to create gathers on a dress. Basically you stich the fabric with a loose stitching number on the sewing machine, you leave 4-6 inches of thread loose at the end and leave it loose then pull it from both sides.
 
· Gauging: gauging means a big piece of fabric made small with shirring the fabric. Loose Stiches rows and pull at the end to gauge the fabric.

· 
· Whipping:  rolled edge to whip a little by little. Wrong side facing you. So the finishing will be on the right side of the garment. 

3. Explain the following types of seams and where each of the following seam is used.
-whipped seam: whipped seam is rolling the edge of the fabric to whip it continuously to attach a fabric piece to another. 

Curved seam: curved seam is used on patterns with a curve. When stitched together after finishing the stitch on it. You will have to make cuts next to the seam to create shape in the garment.

Strap seam: strap seam is used for decoration on a garment. Usually seen on outer side of the zip area. Or neckline etc. 

Lapped hem stitched seam: seams lapped one over the other. Wrong side to the right side. Usually a form of top stitching.

Tucked seam: A stitched fold of fabric, used for a decorative look or to shape a garment.
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