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                                                       ENIRONMENTAL IMPACT STUDY 



 In the pre-build and site determination the impact must be assessed on the site area and the surrounding conurbation to determine to see if it would be 

Compatible to move forward with the project .

The type of build is another major issue houses next to houses is very different to a factory next to houses

Or a shopping centre. 

So what are negative factors lets start with traffic management it’s a big player houses to houses one if not two cars per house maybe more 

If this is a village setting maybe small roads speeding noise air quality parking problems are a few impacts 

Houses next to a factory or vice versa large vehicles in and out all the work force coming and going .noise light pollution maybe 24 hour 

Operating 7 days a week the list could go on and on so to limit any of these or to rule out altogether can save a great deal of red tape 

And cost .committee meetings locals protesting councils well anyone or anything that maybe impacted by the said development 

Is classed as an impact .

                                                     BASIC CRITERION



When a commercial building or factory project that requires a fair size work force the area under consideration will look to this being close

To hand and qualified enough 

Topographical surveys are under taken to work out the physical demographic of site suitability .

Very undulating land soil conditions maybe trees with T.P.O.on them (tree presevation order)    

Difficult access and such like climate is also a consideration more so in areas that are prone to very large fluctuations in temperature 

And humidity ,wind rain major elements to be aware of .

To achieve the delivery of basic services to the site is a element not to be taken lightly .water power ,drainage , raw materials .

Although some of this can be managed off grid with solar power or generators .sedimenter tank for waste . rain harvesting or bowser

If necessary .

But still the main factor and the main concern always is cost for all aspects outlined .



                                                                    

                                                      TOPOGRAPHIC

                                                       



This is the lay of the land to be considered .the datum is sea level ^ so the servey will tell you of the rise and fall of the land within the plot

0-------!0% for an example more geographical information includes all water courses and ground that is very problematic trees over 6 inches 

In diameter will be placed on  and the root area shown .all the boundaries of the site will be ordnance servey for accuracy .

   

                                                        BED ROCK



Bed rock very hard and non-porous element very good for heavy structures . bridges ,viaducts,  ,power stations dams and tunnels would 

All benefit from this type of foundation .years ago most castles were cited on bed rock not only to hold the weight but also for the building material 

This maybe good for these heavy buildings but not good to work with on smaller construction very difficult to work with .
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                                                                       CLASSIFICATION OF BUILDINGS 



A)   MUSEUM 

CLASS  D-NON REIDENTIAL INSTITUTIONS      CLASS D-1











HOSPITAL

CLASS C2 IS THE MAIN CLASS BUT ALSO D 1  FOR MEDICAL OR HEATH WHERE THE 

PRACTITIONERS DOES NOT RESIDE 





HOTEL

CLASS C  C-1





LIBRARY #

CLASS D   D-1 



DEPARTMENT STORE

CLASS  A  A-1
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