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Marking Criteria:
 We expect the learners to write minimum one well expressed point in three lines against each allocated mark. This means one needs to write 15 lines with 5 well expressed points to get high grades for a 5 marks question.
For high grades use examples and illustrations where appropriate. 
	
1. 	Answer the following questions: 	 	 	 	 	 	 	 	(20) 
 
i. What are the economic objectives of quality control and how are they achieved?  

Every construction project seeks to build a structure at the least cost of high quality. A high quality structure can be achieved at lower cost if the following costs are minimized or reduced:
· Failure cost due to quality issues with materials or products which may result in rework, scrapping, low productivity on the field or even spoilage of items.
· Appraisal cost inherent in conducting quality control assurance using testing, inspection and other means of product evaluation.
· Prevention costs associated with avoiding mistakes during construction. The costs are linked to personnel training, quality control engineering and maintenance of equipment.
Some economic reasons for undertaking quality control include:
· Cost savings by minimizing rejects or rework.
· Cost savings by keeping within boundary of design specifications and not extending beyond.
· Savings obtained by making quality product at no extra cost to parties involved in the project.
Savings will happen when the contractor engages the services of well-trained supervisors. 

ii. What are the features of field quality control?  

Field quality control requires the use of equipment, employees’ expertise and other facilities depending on the quality measure stipulated in the contract. It is responsibility of the lab manager to evaluate equipment requirements and deployment during quality control checks. The number of personnel required to perform quality control inspection and testing will depend on the workload and scheduling of activities on the field. It is best to wait and perform quality control measurements after the peak periods of activities when more workers become available. To ensure quality control measures are effectively, it is important to perform priority ratings for each activity to differentiate between the most and least vital activities. Priority is given to activities having the highest rating first when carrying out quality control procedures.
Field quality control usually involves:
· The desire to provide an excellent service
· Discovering the most effective way of performing tasks
· Making use of experience to get things done
· Being proud of effort one makes to get tasks accomplished
· Providing business opportunity for the contractor
· The owner getting joy and satisfaction from having value for money.

iii. 	How can contractor quality control be implemented effectively?

Quality control personnel undertake checks on the field activities to ensure that the contractor is complying with quality standards according to the design specifications. 
The contractors’ quality control plan is vital to assure the project owner(s) that everyone involved is aware of the steps needed to achieve a high quality product. The quality control plan of the contractor is usually discussed by all participants before work begins. It is neither meant to control activities of the contractor nor to pry into his affaires but to endure everybody understand why it is important to maintain good quality control measure at all time. 

 iv. 	Why are specifications important?  

Specification deals with the quality of work being undertaken in the field using the right quality of materials. Limits are set on the physical properties of materials for quality control purposes. If a quality control inspector finds that a representative sample of a particular material being tested or evaluated falls outside the specified limits, the material from which the sample was taken may be rejected if successive tests show all results are outliers or fall outside the limits.
It is the prerogative of the designer to specify what is an acceptable or an unacceptable result from the beginning. Statistical and probability tools may be used for evaluation of samples and determining the quality of materials being used on the field. When a sample falls outside specifications, the whole batch or lot from which it was taken may be rejected.

v. 	What are incentives and penalties in specifications? 

Restrictions are normally imposed on the contractors to prevent them from rushing to complete the project ahead of schedule. This safeguard the project in terms of quality control objectives as specified in the contract. Penalties in the form of fines are sanctioned against the contractor if he fails to follow the specified procedures. Incentives are provided for compliance with laid down procedures. Both penalties and incentives are included in contracts, but it is advisable to avoid including penalties because they tend to strain the relationship between the owner and the contractor.
 
2. How can you achieve quality control in the field?  	(5)   

· Develop the necessary technical and practical expertise that will be required to specify quality requirements for each activity and facility
· Creating clear and accurate designs, drawings, specification and models which will translate into quality products on the field
· Having the contractor’s field management personnel take part in the design process and quality control specifications
· Spearheading procurement of only quality materials
· Ensuring measures are in place to protect equipment and materials during all phases of construction
· Researching effective methods of construction using suitable equipment and tools
· Developing and using the latest quality control technology and know-how to function effectively
· Making contractor understand the need for quality control and making sure his staff are trained to ensure the highest quality on the field
· Providing assistance to establishing quality control on the job site
· Frequent visits to the site to ensure quality control program are being executed and also collaborating with field staff to solve quality control problems
· Making available engineer with enough experience to deal with quality control issues
· Ensuring that the contractor explains to subcontractors all of their responsibility and the objectives of the project
· Keeping effective records of issues and providing feedback to design engineers to help future projects avoid such issues
· Getting design personnel involved in providing solutions to problems arising in the field of construction.
	 	 	 	 
What are the advantages and disadvantages of contractor quality control'? (5)

· When testing and inspection are integral part of the project, then the cost can be well-managed by the contractor
· The contractor is in a stronger position to anticipate problems and take the necessary steps to adjust the work to solve the problem
· The contractor is better placed to build quality into the product than the owner’s quality control supervisor
· Testing by the contractor can help him improve on his performance or efficiency at relatively lower cost
· Integrating statistical specification into the contractor’s daily activity and displaying this information for other workers to view on daily basis will yield better overall quality
· Disputes between the contractor, suppliers and quality control department may be avoided if all quality issues are made the sole responsibility of the main contractor
· There will be more time available to the owner’s quality control team to focus on solving more general problems on the site.
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